If distance<=20cm

Initialize ultrasonic sensor,servo motor, motor driver

Read distance

Move stop

Move backward

Move stop

Look right

Read right distance

Look left

Read left distance

Turn left

no

Move forward

yes

Move stop

If right distance>=left distance

yes

Turn right

no